SETTING THE -TIMER

Connect the THE-Timer to a 6 volt **Alkaline OR LITHIUM** battery using the alligator clips. If you are using a rechargeable style battery, you may disconnect the alligator clips and use the ¼” quick connects. **NEVER USE A CARBON -ZINK 6 VOLT, OFTEN SOLD AS HEAVY DUTY OR SUPER HEAVY DUTY**. These batteries do not last in the Stable Grazer.

1.Push **Set Clock**

2. Push/Use the **Hr.** & **Min** buttons to the correct time of day. (Make sure the Am/PM settings are correct throughout programming.

3. Push **Run Time** button, set run time to 2 seconds. (This programs the run time for the **Test** button)

4. Push **P1** to begin programming your first feeding

* Use **Hr.** & **Min** buttons to program the desired time you for your first shelf drop (feeding)
* Use **Run Time** button, set the run time to 2 seconds.

Repeat step 4 for P2 (2nd feeding) through P6 (6th feeding)

5.To test or reset bottom cam position push the **Test** button.

**IMPORTANT!**

If the bottom shelf does not lock into position, the feeder is out of time. Press the test button to reset the cam.

HayDay,LLC www.stablegrazer.com